## Front Fender Fairing Replacement

1. | Remove the front inner fender as necessary.

2. | Open the front door. From inside the door, remove the clips securing the front fender fairing (A) and front fender.

3. | From the wheel arch, remove the clip (A), and release the clip (B), then remove the front fender fairing (C).

4. | Install the fender fairing in the reverse order of removal, and note these items: Replace any damaged clips. Before installing the clips of the door upper and lower portions, install the front fender fairing to the front fender (D) properly as shown.