## Injector Replacement

1. | Relieve fuel pressure.

2. | Remove the air cleaner.

3. | Remove the intake manifold.

4. | Disconnect the connectors from the injectors (A), and remove the harness clip (B) from the fuel rail (C).

5. | Disconnect the quick-connect fittings (D).

6. | Remove the fuel rail bracket (E).

7. | Remove the fuel rail mounting nuts (F) from the fuel rail.

8. | Remove the injector clip (G) from the injector.

9. | Remove the injector from the fuel rail.

10. | Coat the new O-rings (A) with clean engine oil, and insert the injectors (B) into the fuel rail (C).

11. | Install the injector clip (D).

12. | Coat the injector O-ring (E) with clean engine oil.

13. | To prevent damage to the O-rings, install the injectors in the fuel rail first, then install them in the injector base (F).

14. | Install the fuel rail mounting nuts. Install the fuel rail bracket (G).

15. | Connect the quick-connect fittings.

16. | Connect the connectors on the injectors, and install the harness clip (H).

17. | Install the intake manifold.

18. | Install the air cleaner.

19. | Turn the ignition switch ON (II), but do not operate the starter. After the fuel pump runs for about 2 seconds, the fuel pressure in the fuel line rises. Repeat this 2 or 3 times, then check for fuel leakage.