## Steering Angle Sensor Replacement

NOTE: Do not damage or drop the combination switch as the steering angle sensor is sensitive to shock and vibration.

1. | Remove the steering wheel, and steering column cover.

2. | Remove the combination switch assembly.

3. | Remove the combination light switch (A) and the wiper/washer switch (B).

4. | Replace the combination switch body complete (C).

5. | Install the combination switch in the reverse order of removal. NOTE: Do not remove the steering angle sensor from the combination switch body.