## Power Window Master Switch Test

1. | Remove the power window master switch.

2. | Disconnect the 20P connector from the switch.

### Driver's Switch:

The driver's switch is combined with the control unit so you cannot isolate the switch to test it.
Instead, run the master switch input test procedures on page 22-122. If the tests if the tests are normal, the driver's switch must be faulty.

Front passenger's Switch:

Left Rear Switch:

Right Rear Switch:

3. | If the switch is faulty, replace the switch.