## Ceiling Light Test/Replacement

1. | Turn the light switch OFF.

2. | Carefully pry off the lens (A) with a small screwdriver.
Ceiling Light: | 8 W

3. | Remove the two mounting screws.

4. | Disconnect the 3P connector (B) from the housing (C).

5. | Check for continuity between the terminals in each switch position according to the table.

6. | Install the light in the reverse order of removal.