## High/Low Beam Switching Solenoid Replacement

1. | Remove the headlight.

2. | Remove the HID bulb from the headlight.

3. | Disconnect the 2P connector (A) from the high/low beam switching solenoid (B).

4. | Turn the headlight adjuster (C) about eight turns counterclockwise.

5. | Place a clean shop towel or paper (D) under the high/low beam switching solenoid.

6. | Remove the two screws from the high/low beam switching solenoid (A).

7. | Disconnect the 1P terminal (B) and remove the high/low beam switching solenoid. NOTE: Do not touch the hood and the moving part. It is necessary to clean if touch the parts.

8. | Install the switching solenoid in the reverse order of removal.

9. | After replacement, check the hood operation and adjust the headlight.