## Heater Control Panel Removal and Installation

NOTE: LHD type is shown, RHD type is symmetrical.

1. | Remove the center panel.

2. | Remove the audio unitor the navigation unit.

3. | Remove the dials (A), then remove the self-tapping screws and the heater control panel (B).

4. | Install the control panel in the reverse order of removal, and note these items: Adjust the air mix control cable, the mode control cable, and the recirculation control cable. After installation, operate the control panel controls to see whether it works properly.