## DTC Troubleshooting: 97

DTC 97: | VSA System

1. | Check for other DTCs. Is another DTC indicated? YES - Do the appropriate troubleshooting for the DTC.n NO - Go to 2.

2. | Clear the DTCs using the HDS.

3. | Test-drive the vehicle at 10 km/h (6 mph) with straight.

4. | Stop the vehicle, and retest-drive the vehicle again.

5. | Verify the DTC. Is DTC 97 indicated? YES - Replace the VSA modulator-control unit.n NO - The system is OK at this time.n