## Fuse to Components Index

Under-hood Fuse/Relay Box
Fuse Number | Amps | Wire Color | Component(s) or Circuit(s) Protected
--- | --- | --- | ---
1 | 80A | ——— | Battery, Power distribution
2 | 40A | WHT/BLU | EPS control unit
3 | 50A | WHT | Ignition switch (BAT)
4 | 40A | WHT/RED | ABS modulator-control unit
5 | 40A | WHT/BLU | Blower motor
6 | 40A | WHT | No. 2, 3, 4, 13 and 14 fuses (in the under-dash fuse/relay box)
7 | 30A | BLU/RED | Power mirror defogger, Sunroof motor
8 | 15A | WHT/RED | Audio unit, Ceiling light, Data link connector, Gauge assembly, Immobilizer control unit-receiver, Immobilizer code unit, Keyless receiver unit, Navigation unit, Spotlights, Tailgate light
9 | 10A | RED/BLK | Dash lights, Front parking lights, Gauge lights, License plate lights, Taillights
10 | 20A | BLU/BLK | Radiator fan motor
11 | 30A | BLU/YEL | A/C compressor clutch relay
BLU/RED | Condenser fan motor
12 | 20A | RED | Right headlight
13 | 20A | RED/YEL | High beam indicator light, Left headlight
14 | 10A | WHT/BLK | Turn signal/hazard flasher control circuit (Has built into gauge assembly)
15 | 30A | WHT/GRN | ABS modulator-control unit
16 | 15A | WHT/GRN | ABS modulator-control unit, Brake lights, ECM/PCM, Shift lock control circuit (Has built into gauge assembly)
BLU/RED | Horn
Fuse/relay box socket | Horn relay

Under-dash Fuse/Relay Box
Fuse Number | Amps | Wire Color | Component(s) or Circuit(s) Protected
--- | --- | --- | ---
1 | ——— | ——— | Not used
2 | 20A | GRN/WHT | Driver's power window motor
3 | 20A | WHT | Door lock actuator, Tailgate lock actuator
4 | 20A | YEL/BLU | Right rear power window motor
5 | 10A | YEL | A/T reverse relay, Back up lights, Rear fog light, Turn signal/hazard flasher circuit (has built into gauge assembly)
6 | ——— | ——— | Not used
7 | 15A | BLK/WHT | Ignition coil (front)
8 | 15A | YEL/GRN | Cigarette lighter
9 | 15A | BLK/RED | Ignition coil (rear), OPDS unit
10 | 20A | GRN/BLK | Rear wiper, Intermittent control unit, Rear washer motor, Windshield wiper motor, Windshield washer motor
11 | 15A | BLK/YEL | ECM/PCM, Fuel pump, Inertia switch, SRS unit (VA)
12 | 20A | BLK/ORN | Rear window defogger
13 | 20A | YEL/RED | Left rear power window motor
14 | 20A | GRN/BLK | Front passenger's power window motor
15 | 10A | PNK | SRS unit (VB)
16 | 7.5A | YEL | Alternator, ABS modulator control unit, EPS control unit, ELD unit, EVAP canister purge valve, Gauge assembly, Headlight adjuster, Headlight adjuster switch, Immobilizer code unit, Keyless receiver unit, Primary HO2S, Sunroof control unit (KU, KT and KK models), Shift lock solenoid (CVT), Secondary HO2S, Vehicle speed sensor (M/T)
17 | 7.5A |  | Audio unit (without navigation), Key interlock control circuit (has built into gauge assembly), Key interlock solenoid, Navigation unit
Fuse/relay box socket | Optional connector
18 | ——— | ——— | Not used
19 | ——— | ——— | Not used
20 | 15A |  | CKP sensor, TDC sensor, ECM/PCM, Injectors, IAC valve, PGM-FI main relay 1, PGM-FI main relay 2
21 | 10A |  | Power window control unit, Rear window wiper motor
Fuse/relay box socket | Power window relay
22 | 7.5A | BLK/YEL | A/C compressor clutch relay, A/C switch, Blower motor relay, Condenser fan relay, Heater control panel, Power mirror actuator, Power mirror defogger relay, Radiator fan relay
Fuse/relay box socket | Optional connector
23 | ——— | ——— | Not used