## Climate Control Unit Removal and Installation

1. | Remove the center panel.

2. | Remove the audio unit.

3. | Remove the dials (A), then remove the self-tapping screws and the climate control unit (B).

4. | Install the control unit in the reverse order of removal, and note these items: Adjust the recirculation control cable. After installation, operate the control unit controls to see whether it works properly.