## Front Bumper Lower Grille Replacement

## Normal Type

NOTE:

- Take care not to scratch the front bumper.
- When prying components, use the handy remover set or equivalent.

1. | Remove the front bumper.

2. | Remove the bumper lower grille (A):
-1 | Remove the screws (B) and clips (C) from the back of the front bumper (D).
-2 | Remove the bumper lower grille from the bumper by releasing all of the hooks (E).

3. | Install the grille in the reverse order of removal. Push the hook portions into place securely.