## CVT Differential Oil Seal Replacement

Special Tools Required
Handle driver ( 07749-0010000)

Driver attachment, 78 x 80 mm ( 07NAD-PX40100)
Driver attachment, 58 mm ( 07JAD-PH80101)

1. | Remove the oil seal from the transmission housing.

2. | Remove the oil seal from the flywheel housing.

3. | Install the new oil seal flush with the transmission housing with the special tools.

4. | Install the new oil seal flush with the flywheel housing with the special tools.