## Roof Molding Replacement

1. | Apply protective tape to the body (A). Using a flat-tip screwdriver wrapped with protective tape (B), pry up on the roof molding (C). Take care not to scratch the body.

2. | Pull up and slide the roof molding to release the front bracket (D) from the pin (E).

3. | Pull up the front portion of roof molding.

4. | Pull up and release the rear bracket (A) from the pin (B), then remove the roof molding (C).

5. | Install the molding in the reverse order of removal, and note these items: Take care not to damage the windshield molding. Make sure the roof molding is installed securely.