## Spotlights Test/Replacement - Without Sunroof

1. | Turn the light switch OFF.

2. | Carefully pry off the lenses (A) with a small screwdriver.
Spotlight: | 8 W x 2

3. | Remove the two mounting screws.

4. | Disconnect the 2P connector (B) from the housing (C).

5. | Check for continuity between the terminals in each switch position according to the table.

6. | Install the light in the reverse order of removal.