## Immobilizer Control Unit-Receiver Replacement

1. | Remove the dashboard lower cover.

2. | Remove the steering column covers.

3. | Disconnect the connectors (A) from the immobilizer control unit-receiver (B).

4. | Remove the two screws and the immobilizer control unit-receiver from the ignition key cylinder (C).

5. | Install the immobilizer control unit-receiver in the reverse order of removal.

6. | After replacement, register the immobilizer control unit-receiver with HDS, then check the immobilizer system.