## M/T Differential Oil Seal Replacement

Special Tools Required
Driver ( 07749-0010000)

Pilot, 26 x 30 mm ( 07JAD-PH80200)
Driver attachment ( 07JAD-PN00100)

1. | Remove the differential assembly.

2. | Remove the oil seal (A) from the transmission housing (B).

3. | Remove the oil seal (A) from the clutch housing (B).

4. | Install the new oil seal (A) in the transmission housing (B) with the special tools.

5. | Install the new oil seal (A) in the clutch housing (B) with the special tools.