## DTC Troubleshooting: P0324 (136)

DTC P0324: | Knock Control System Error

1. | Turn the ignition switch ON (II).

2. | Do the DTC CLEAR in the CLEAR MENU with the HDS.

3. | Turn the ignition switch OFF.

4. | Turn the ignition switch ON (II).

5. | Check for Temporary DTCs or DTCs in the DTCs MENU with the HDS. Is DTC P0324 indicated? YES - Substitute a known-good ECM and recheck. If symptom/indication goes away, replace the original ECM.n NO - Intermittent failure, system is OK at this time.n