## Driver's Dashboard Under Cover Removal/Installation

NOTE:

- Take care not to scratch the dashboard and related parts.
- LHD is shown, RHD is symmetrical.

1. | Remove the driver's dashboard under cover (A).
-1 | Turn the lock knob (B) 90°.
-2 | Gently pull down the rear edge to release the clip.
-3 | Pull the cover away to release it from the clip (C) on the body and to release its pin (D) from the kick panel (E).

2. | Install the cover in the reverse order of removal.