## Ceiling Light/Spotlights Test/Replacement - With Sunroof

1. | Turn the ceiling light/spotlights switches OFF.

2. | Carefully pry off the lens (A) with a small screwdriver.
Ceiling Light: | 5 W
Spotlight: | 5 W x 2

3. | Remove the two screws and the housing (B).

4. | Disconnect the 4P connector (C) from the housing.

5. | Check the bulbs. If the bulbs are OK, check for continuity between the terminals in each switch position according to the table.

6. | Install the light in the reverse order of removal.