## Outside Air Temperature Sensor Test

1. | Remove the outside air temperature sensor.

2. | Dip the sensor in ice water, and measure the resistance. Then pour warm water on the sensor, and check for a change in resistance.

3. | Compare the resistance reading between the No. 1 and No. 2 terminals of the outside air temperature sensor with the specifications shown in the graph; the resistance should be within the specifications.

4. | If the resistance is not as specified, replace the out side air temperature sensor.