## Fuse to Components Index - Suppelemnt

Under-hood Fuse/Relay Box
Fuse Number | Amps | Wire Color | Component(s) or Circuit(s) Protected
--- | --- | --- | ---
1 | 80A | ——— | Battery, Power distribution
2 | 40A | WHT/BLU | EPS control unit
3 | 50A | WHT | Ignition switch (BAT)
4 | 40A | WHT/RED | ABS modulator-control unit
5 | 40A | WHT/BLU | Blower motor
6 | 40A | WHT | No. 2, 3, 4, 13 and 14 fuses (in the under-dash fuse/relay box)
7 | 30A | BLU/RED | No.24 fuse (in the auxiliary fuse holder) (with front fog light), Power mirror defogger, Sunroof motor
8 | 15A | WHT/RED | Audio unit, Ceiling light, Data link connector, Gauge assembly, Immobilizer control unit-receiver, Immobilizer code unit, Keyless receiver unit, Navigation unit, Spotlights, Tailgate light
9 | 10A | RED/BLK | Dash lights, Front parking lights, Gauge lights, License plate lights, Taillights
10 | 20A | BLU/BLK | Radiator fan motor
11 | 30A | BLU/YEL | A/C compressor clutch relay
BLU/RED | Condenser fan motor
12 | 20A | RED | Right headlight
13 | 20A | RED/YEL | High beam indicator light, Left headlight
14 | 10A | WHT/BLK | Turn signal/hazard flasher control circuit (Has built into gauge assembly)
15 | 30A | WHT/GRN | ABS modulator-control unit
16 | 15A | WHT/GRN | ABS modulator-control unit, Brake lights, ECM/PCM, Shift lock control circuit (Has built into gauge assembly)
BLU/RED | Horn
Fuse/relay box socket | Horn relay

Auxiliary Fuse Holder
Fuse Number | Amps | Wire Color | Component(s) or Circuit(s) Protected
--- | --- | --- | ---
24 | 20A | BLU/BLK | Front fog lights

Fuse Number | Amps | Wire Color | Component(s) or Circuit(s) Protected
--- | --- | --- | ---
25 | 7.5A | YEL | ABS modulator-control unit