## DTC Troubleshooting: 6

DTC 6: | A Short in the Sunlight Sensor Circuit

1. | Disconnect the sunlight sensor 2P connector.

2. | Disconnect climate control unit connector.

3. | Check for continuity between the No. 9 terminal of climate control unit connector A (12P) and body ground. Is there continuity? YES - Repair short to body ground in the wire between the climate control unit and the sunlight sensor.n NO - Go to 4.

4. | Reconnect the sunlight sensor 2P connector.

5. | Reconnect climate control unit connector A (12P).

6. | Test the sunlight sensor. Is the sunlight sensor OK? YES - Substitute a known-good climate control unit, and recheck. If the symptom/indication goes away, replace the original climate control unit.n NO - Replace the sunlight sensor.n