## Brake Hoses and Lines Inspection

1. | Inspect the brake hoses, for damage, deterioration, leaks, interference, and twisting.

2. | Check the brake lines for damage, rusting, and leakage. Also check for bent brake lines.

3. | Check for leaks at hose and line joints or connections, and retighten if necessary.

4. | Check the master cylinder and ABS modulator unit (if equipped) for damage and leakage. NOTE: Replace the brake hose clip whenever the brake hose is serviced.